\section{Edge folding device}
\textbf{Tujuan}
\begin{itemize}
    %<*tujuan>
    \item Menggunakan komponen tunda waktu
          %</tujuan>
\end{itemize}
\ifdef{\showhiden}
{
    \textbf{Kesimpulan}
    \begin{enumerate}
        %<*kesimpulan>
        \item Komponen tunda waktu adalah valve/ timer yang dapat berubah kondisinya
              setelah waktu yang dapat diatur.
              %</kesimpulan>
    \end{enumerate}
}{}
\textbf{Deskripsi Perangkat}
\begin{itemize}
    \item silinder-double acting mendorong benda kerja berbentuk tabung seperti ilustrasi dibawah.
          benda kerja akan dipisahkan dengan cara silinder digerakkan maju-mundur secara terus menerus.
    \item kecepatan memanjang silinder lebih lambat dari memendek
    \item silinder akan tetap memanjang dengan tunda waktu selama 1 detik
\end{itemize}

\begin{center}
    \begin{tabular}{p{.5\textwidth} p{.5\textwidth}}
        \begin{tabular}{|p{.4\textwidth}| p{.04\textwidth}|} \hline
            \textbf{Komponen Umum}                 & \textbf{N} \\ \hline
            Service unit with on-off valve         & 1          \\
            Manifold                               & 1          \\
            Double-acting cylinder                 & 1          \\
            One-way flow control                   & 2          \\ \hline
            \textbf{Komponen Pneumatic}            & \textbf{N} \\ \hline
            Two preassure valve                    & 1          \\
            5/2-way impulse pneumatically operated & 1          \\
            3/2-way, manual operated               & 1          \\
            Pneumatic timer                        & 1          \\
            3/2-way valve with roller lever        & 2          \\ \hline
            \textbf{Komponen Electropneumatic}     & \textbf{N} \\ \hline
            5/2-way impulse solenoid valve         & 1          \\
            Relay                                  & 1          \\
            Relay with switch-on delay             & 1          \\
            pushbutton (make)                      & 1          \\
            make switch                            & 2          \\
            make switch-roller                     & 2          \\
            Electrical power supply unit, 24 V     & 1          \\ \hline
        \end{tabular} &
        \includegraphics[scale=.35]{Screenshot_2021-04-08_12-39-45.png} \\
    \end{tabular}
\end{center}
\subsubsection{Tugas Praktik}
\input{tugas_praktek.tex}
\subsubsection{Evaluasi}
\begin{enumerate}
    \item Ceritakan cara kerja rangkaian yang telah dipraktikkan apabila terpasang pada perangkat sebenarnya!
          %<*pemantik>
    \item Apa perbedaan dari one-way flow control dengan valve tunda waktu?
          %</pemantik>
\end{enumerate}
\newpage
\subsubsection{JAWABAN}
\textbf{Gambar Rangkajian}\\
\ifdef{\drawCircuit}{
    \begin{tabular}{p{.5\textwidth} p{.5\textwidth}}
        Pneumatic                                        & Electropneumatic \\
        \includegraphics[scale=.5]{2022-08-29_12-42.png} &
        \includegraphics[scale=.5]{2022-08-29_12-42_1.png}                  \\
    \end{tabular}
}{
    \ifdef{\drawPartialCircuit}{
        \begin{tabular}{p{.3\textwidth} p{.7\textwidth}}
            Pneumatic                                        & Electropneumatic \\
            \includegraphics[scale=.5]{2022-08-29_12-45.png} &
            \includegraphics[scale=.6]{2022-08-29_12-44.png}                    \\
        \end{tabular}
    }{
        \vspace{4cm} \\
    }
}
\input{perbandingan_langkah_pergerakan.tex}
